PRESS RELEASE

**Get well soon**

**Public hospital in Solothurn with user-focused glass solutions from Glas Trösch**

**Bützberg (CH), October 2021.** *A new 290-bed public hospital recently open its doors in Solothurn, Switzerland. The striking base structure as well as the patients’ ward above it are fitted with triple insulating glass by Glas Trösch, which creates an ideal room climate. Inside, around 3.5 kilometres of glass partition walls and doors were used, which let in natural light while fulfilling functions such as fire protection, privacy and noise protection. In their design, the consultants at Silvia Gmür Reto Gmür Architekten are meeting the current demand of hospitals for consistent focus on people’s needs.*

The history of the Solothurn Public Hospital goes back as far as the year 1418. The hospital was last housed in a typical concrete building erected in the 1970s. Having reached its capacity limits for quite some time, however, the hospital held an international architecture competition for a new building in 2008. The contest was won by Silvia Gmür Reto Gmür Architekten with their design for an L-shaped base structure surmounted by a six-storey high-rise building. This solution won over the competition jury not only from an operational standpoint, but also from an urban planning perspective.

**Generous glazing in the public areas**

The public, examination and treatment areas are located in the two-storey base structure. Here, the building is developed along the facades. This creates an area of around 5,700 square metres per floor which accommodates the medical departments. Bright corridors running on the perimeter allow patients, visitors and staff to view the surrounding landscape. With its scale-like structure, the facade helps create high quality amenities in every zone. Above all, the extensively glazed, eight-metre-high mullion and transom facade also contributes to this effect.

The triple glazing in the SILVERSTAR SUPERSELEKT 35/14 T execution supplied by Glas Trösch, which offers very efficient summer heat protection with a g-value of only 12 percent, ensures comfort inside the building. It was therefore possible to dispense with external shading, which gives the base structure a clear and distinctive appearance.

**Ideal climate in the patient rooms**

The patients’ ward marks the intersection of the two wings of the L-shape. Here, the facade has a more delicate appearance. The curtain-type shading system, which consists of 1,740 sculptural elements made of white concrete, has a particularly distinctive effect. The actual facade behind it consists of floor-to-ceiling full glazing. Here, too, triple insulating glass by Glas Trösch was selected, but with a different functionality than in the case of the base structure: SILVERSTAR COMBI Neutral 51/26 was used, which combines basic heat protection with very good thermal insulation. The latter is improved even further by an additional coating and thus achieves an extremely low Ug value of 0.51 W/m²K with an impressive 44.5 percent light transmission. All in all, this generates optimal conditions for the speedy recovery of the patients, who can enjoy remarkably good views of the countryside thanks to the high colour neutrality of the glass. The ensuing focus on the patient’s needs, called “Healing Architecture” by the architects, makes the architecture part of the therapy.

**3.5 kilometres of glass partitions**

Inside the new building, partition walls from the Swiss specialist BlessArt were installed, which are fitted with SWISSDUREX tempered safety glass supplied by Glas Trösch. The 3.5 kilometres of partition walls and around 500 doors ensure that the rooms are flooded with natural light and meet a wide range of requirements: from a particularly high level of sound insulation in the sleep laboratory, effective radiation protection in radiology to reliable fire protection in the corridors. What all walls have in common is that they are particularly hygienic, robust and easy to care for by using glass as a material. They are also impressive in terms of design, because of their different print and paint finishes.

**High energy savings standards**

Solothurn Public Hospital was the first hospital in Switzerland to be certified according to the Minergie-ECO standard, which also explicitly takes into account the aspects of “daylight” and “indoor climate”. The glass solutions played a significant part in achieving this high building standard. The building won the prestigious “best architects award” in 2021.

The first construction phase was launched in the middle of this year, and construction phase 2 is scheduled for completion in 2026.

**Construction panel:**

Project: Solothurn Public Hospital

Location: Solothurn, Switzerland

Completion: 2020

Owner: Canton of Solothurn, Rötihof Public Works department, Solothurn

Architects: Planergemeinschaft Bürgerspital Solothurn, Silvia Gmür Reto Gmür Architekten, Basel

Construction site management: Planergemeinschaft Bürgerspital Solothurn, Walter Dietsche

Baumanagement AG, René Wieland

Facade design: PPEngineering GmbH, Basel

Products: Triple insulating glass SILVERSTAR SUPERSELEKT 35/14 T with an additional coating of SILVERSTAR EN2plus

Triple insulating glass SILVERSTAR COMBI Neutral 51/26 with an additional coating of SILVERSTAR ZERO Eplus

Glass partition system supplied by BlessArt Raumsysteme AG, made with Glas Trösch SWISSDUREX tempered safety glass

**Figures:**



The new public hospital in Solothurn with Glas Trösch facade glass solutions.

Photo: Glas Trösch



Highly efficient heat protection was important for the glazing of the base structure,

which is achieved with triple insulating glass from Glas Trösch.

Photo: Glas Trösch



The examination and treatment areas of the base structure overlook a green

inner courtyard.

Photo: Glas Trösch



The high colour neutrality of the SILVERSTAR COMBI Neutral triple insulating

glass ensures that conditions are optimal for the patient’s speedy recovery.

Photo: Ralph Feiner



Inside Solothurn Public Hospital, too, glass is omnipresent: Transparent and

translucent walls and doors ensure rooms are flooded with natural light.

Photo: BlessArt Raumsysteme AG



The partition walls and doors supplied by BlessArt are fitted with Glas Trösch

glass solutions which fulfil different functions while creating a visually striking effect.

Photo: BlessArt Raumsysteme AG

**Further Information:**

Barbara Sollberger | Glas Trösch Holding AG

Head of Marketing Architectural Glass

Industriestrasse 29, CH-4922 Bützberg

Tel. +41 (0) 62 958 52 46 | [b.sollberger@glastroesch.ch](mailto:b.sollberger@glastroesch.ch)

**Answers to press inquiries:**

Johanna Schulz | Matthias Mai

mai public relations GmbH

Leuschnerdamm 13 | D-10999 Berlin

Tel. +49 (0) 30 66 40 40 554 | [glas\_troesch@maipr.com](mailto:glas_troesch@maipr.com)