## MEDIA RELEASE

**The flush-mounted glass railing system for purist architecture**

**SWISSRAILING FLAT from Glas Trösch**

**Bützberg, March 2020.** When planning balconies and loggias, the choice of balustrade plays a crucial role. Although safety is of paramount concern, balustrades should also serve to enhance the architectural appearance of the building. Here, systems featuring laminated safety glass offer suitable solutions for every area of application. As a transparent and robust material, glass affords a view in either direction. Furnished with a tint or textured surface, it adds a special touch and provides protection against prying eyes. At the same time, it always appears light and elegant. This is especially true for the new SWISSRAILING FLAT all-glass railing system from Glas Trösch. It stands out for its flush-mounted aesthetics thanks to the invisible support structure.

SWISSRAILING FLAT conveys an unadulterated all-glass appearance. In contrast to other solutions, the balustrade glass is bonded directly to the carrier profile – without visible brackets or support structure. Where it overlaps the building, the SWISSLAMEX laminated safety glazing used is printed with a coloured ceramic coating covering the entire surface, precisely colour-coordinated up to the bottom edge of the pane. The result is an exceptionally clean appearance. This effect is further emphasised by incorporating an exposed glass edge, that is to say a handrail-less finish.

**Maximum precision and safety for every type of building**

The SWISSRAILING FLAT concept is based on two profiles, the basic profile and the carrier profile. The latter is already firmly attached to precision-made, customised SWISSLAMEX laminated safety glass at the factory. This high degree of precision optimises the entire installation process, eliminating time-consuming on-site installation work. Although the innovative railing system allows great scope for perfection and adaptation to particular customer specifications, Glas Trösch attaches great importance to the highest standards of safety when combining materials. They are chosen in such a way that they comply with the special requirements for railings and balustrades, including certified fall protection in accordance with the currently applicable standards and guidelines.

Whether for homes, offices or public buildings, whether newly built or renovated – SWISSRAILING FLAT is suited to every type of building. Thanks to its flush-mounted aesthetics, it lends itself especially well to purist architectural solutions with a clear design language.

**Pictures:**



**Glas-Troesch\_SWISSRAILING-FLAT\_1.jpg**

Thanks to its flush-mounted aesthetics, this glass railing system lends itself especially well to architecture with a clear design language. Photo: Glas Trösch

 

**Glas-Troesch\_SWISSRAILING-FLAT\_2.jpg / Glas-Troesch\_SWISSRAILING-FLAT\_3.jpg**

Flush-mounted and simple aesthetics thanks to the invisible support structure. Photo: Glas Trösch

**For further information:**

Bruno Kassnel-Henneberger | Glas Trösch AG Swisswall

Industriestraße 29 | 4922 CH-Bützberg

Tel. +49-(0)821-540 161 26

swisswall@glastroesch.ch | www.glastroesch.ch

**Please address press enquiries to:**

Johanna Schulz | Matthias Mai

mai public relations GmbH

Leuschnerdamm 13 | D-10999 Berlin

Tel. +49-(0)30-66 40 40-550 | glas\_troesch@maipr.com